**Flood Monitoring And Early Warning**

**1.Define Project Requirements and Objectives:**

* Define the specific objectives of your project, such as monitoring water levels, sending alerts, and providing data visualization.

**2. Hardware Setup:**

* Acquire the necessary IoT devices (e.g., water level sensors, microcontrollers like Arduino or Raspberry Pi, and communication modules) and set them up near the flood-prone areas.
* Program the microcontrollers to collect data from sensors.

**3. Data Collection and IoT Integration:**

* Develop code to collect data from the sensors.
* Use technologies like MQTT or HTTP to transmit this data to a cloud-based server or platform.

**4. Cloud-Based Server and Database:**

* Set up a cloud server (e.g., AWS, Azure, or Google Cloud) to receive and store the sensor data.
* Create a database to store historical data.

**5. Backend Development:**

* Build a backend application (using Node.js, Python, or any other preferred language) to process and manage the data.
* Implement algorithms to analyze the data and detect potential flood conditions.

**6. Alerting System:**

* Create an alerting system that sends notifications to users in case of potential flooding.
* Use technologies like Twilio for SMS alerts or email notifications.

**7. Web Dashboard:**

* Develop a web-based dashboard to visualize real-time and historical data.
* Utilize HTML, CSS, and JavaScript for the front-end development.

**8. Map Integration:**

* Integrate maps (Google Maps, Leaflet, or Mapbox) to display sensor locations and flood-prone areas.

**9. User Authentication:**

* Implement user authentication and authorization to restrict access to sensitive data.

**10. Mobile App (Optional):**

* Develop a mobile app using technologies like React Native or Flutter to provide a mobile interface for users.

**11. Testing:**

* Thoroughly test the system to ensure it works as intended, simulating flood conditions if possible.

**12. Deployment:**

* Deploy your web application, database, and backend on a secure web server.

**13. Maintenance and Updates:**

* Plan for regular maintenance, updates, and improvements based on user feedback.

**14. Education and Outreach:**

* Promote awareness about the project within the community and provide information on how residents can access flood warnings.

**15. Data Analysis and Reporting:**

* Create reports and data visualizations to analyze historical flood data, which can be useful for decision-makers and researchers.

**16. Scale the System:**

* Consider expanding the system to cover more areas and integrate additional environmental sensors.

**Creating a mobile app forIoT Flood Monitoring and Early Warning project:**

using Python is a great idea. One of the popular frameworks for developing cross-platform mobile apps in Python is Kivy. Kivy is an open-source Python library for developing multitouch applications, and it works on Android, iOS, Windows, Linux, and macOS. Here's a simple example of how to create a basic mobile app using Kivy for your project:

**Install Kivy**: First, you need to install Kivy. You can do this using pip:

pip install kivy

**create a python program :**

Below is a basic example of a Python program using Kivy to create a mobile app for your project. This app will have a simple interface to display flood sensor data.

from kivy.app import App

from kivy.uix.boxlayout import BoxLayout

from kivy.uix.label import Label

from kivy.uix.button import Button

class IoTApp(App):

def build(self):

# Create the main layout

layout = BoxLayout(orientation='vertical')

# Add a label to display flood sensor data

self.sensor\_data\_label = Label(text="Flood Sensor Data: N/A")

layout.add\_widget(self.sensor\_data\_label)

# Add a refresh button

refresh\_button = Button(text="Refresh Data")

refresh\_button.bind(on\_press=self.refresh\_data)

layout.add\_widget(refresh\_button)

return layout

def refresh\_data(self, instance):

# You can implement code here to fetch and update sensor data from your IoT backend

# For simplicity, let's assume we receive data from a hypothetical API

sensor\_data = self.fetch\_sensor\_data\_from\_api()

self.sensor\_data\_label.text = f"Flood Sensor Data: {sensor\_data}"

def fetch\_sensor\_data\_from\_api(self):

# In a real project, replace this with code to fetch data from your IoT backend

# For this example, we'll just return a mock value.

return "Water Level: 3.2m"

if \_\_name\_\_ == '\_\_main\_\_':

IoTApp().run()

* We create a Kivy app class IoTApp.
* In the build method, we define the app's user interface, which consists of a label to display sensor data and a button to refresh the data.
* The refresh\_data method is called when the refresh button is pressed. You would replace this with code to fetch data from your IoT backend.
* The fetch\_sensor\_data\_from\_api method is a placeholder for fetching sensor data. In a real project, you would make HTTP requests to your server to get the actual data.

**connect with mobile app:**

To connect your mobile app , which you've created using Kivy, with your IoT Flood Monitoring and Early Warning project, you need to establish a communication link between the app and the IoT backend. This typically involves making HTTP requests to your server or IoT platform to retrieve data. Here's a general outline of how you can achieve this:

**Expose an API from Your IoT Backend:**

* 1. Your IoT backend should have an API that the mobile app can communicate with. This API should provide endpoints for retrieving sensor data, alerts, and other relevant information.

**Make HTTP Requests from the Mobile App:**

In your Kivy mobile app, you can use Python libraries like requests to make HTTP requests to the API endpoints of your IoT backend.

import requests

def fetch\_sensor\_data\_from\_api(self):

url = "https://your-iot-backend.com/api/sensor-data"

response = requests.get(url)

if response.status\_code == 200:

data = response.json()

return data

else:

return "Failed to fetch data"

**Handle API Responses:**

* Process the data returned by the API in your mobile app and update the user interface accordingly. For example, you can display sensor data, alert messages, or other relevant information on the app's screens.

**Authentication and Security:**

* Ensure that your API is secure and uses proper authentication methods (e.g., API keys, tokens) to restrict access to authorized users. You should also implement encryption (HTTPS) to protect data transmission between the app and the backend.

**Real-Time Updates (Optional):**

* If you want to provide real-time updates to the app, you can implement technologies like WebSockets or server-sent events (SSE) in your IoT backend. The app can subscribe to these real-time streams to receive immediate notifications about flood conditions.

**Error Handling:**

* Implement error handling in the mobile app to deal with network issues, server unavailability, or other unexpected problems that may arise during data retrieval.

**Testing and Optimization:**

* Thoroughly test the app's communication with the IoT backend to ensure it works as expected. Optimize the app's code and network requests for performance and efficiency.

**User Experience:**

* Consider the user experience by adding features such as push notifications for critical alerts, a user-friendly interface, and options for user preferences.

**Deployment and Distribution:**

* Once your mobile app is ready, you can deploy it to Android and iOS platforms. You may need to go through app store submission processes for distribution.

**PYTHON CODE TO CONNECT WITH WOKWI:**

import time

from machine import Pin, PWM, UART

import dht

import network

import urequests

# Replace with your Wi-Fi network name and password

SSID = "your\_SSID"

PASSWORD = "your\_PASSWORD"

# Replace with your ThingSpeak API key and channel ID

API\_KEY = "your\_API\_KEY"

CHANNEL\_ID = "your\_CHANNEL\_ID"

# Initialize Wi-Fi connection

sta = network.WLAN(network.STA\_IF)

sta.active(True)

sta.connect(SSID, PASSWORD)

# Wait for Wi-Fi connection

while not sta.isconnected():

pass

print("Connected to Wi-Fi")

# Initialize DHT sensor (assuming you're using DHT22)

dht\_sensor = dht.DHT22(Pin(4))

# Initialize PIR sensor

pir\_sensor = Pin(13, Pin.IN)

# Initialize ultrasonic sensor (assuming you're using HC-SR04)

trig = Pin(5, Pin.OUT)

echo = Pin(4, Pin.IN)

# Initialize ThingSpeak URL

TS\_URL = "https://api.thingspeak.com/update"

def read\_ultrasonic\_distance(trig\_pin, echo\_pin):

trig\_pin.on()

time.sleep\_us(10)

trig\_pin.off()

while not echo\_pin.value():

pass

t1 = time.ticks\_us()

while echo\_pin.value():

pass

t2 = time.ticks\_us()

return (t2 - t1) / 58

# Initialize UART for serial communication (for debugging)

uart = UART(0, 115200)

while True:

pir\_value = pir\_sensor.value()

distance = read\_ultrasonic\_distance(trig, echo)

if pir\_value:

Pin(12, Pin.OUT).on()

time.sleep(0.001)

else:

Pin(12, Pin.OUT).off()

if distance <= 100:

pwm = PWM(Pin(6))

pwm.freq(880)

pwm.duty(512)

time.sleep(0.125)

pwm.deinit()

else:

Pin(6, Pin.OUT).off()

dht\_sensor.measure()

temperature = dht\_sensor.temperature()

humidity = dht\_sensor.humidity()

# Send data to ThingSpeak

params = {

"api\_key": API\_KEY,

"field1": distance,

"field2": temperature,

"field3": humidity

}

response = urequests.get(TS\_URL, params=params)


if response.status\_code == 200:

print("Data sent to ThingSpeak successfully")

else:

print("Failed to send data to ThingSpeak")

time.sleep(15)

**circut diagram:**